2015-07-23 Pitch depth of rack, UI improvements

2015-06-01 Improved messaging when creating assemblies in CAD

2015-05-12 AI Published

2015-05-06 More changes to bevel mounting

2015-04-22 Tooth Tip Radius for external spur/helical gears was added
			made the picScreen filled for better resizing with the mouse
			
****End of 2015 enhamcements

2015-04-16 GetSolidEdgeID updated for Surface... all 2015-16 products were updated

2015-04-07 Registration, no longer requires user to input email and company name

2015-04-06 AI helical spur, tooth extrusion when in metric units corrected

2014-12-14 Reverse annimation direction had not been programmed. If normal to cutter was selected, it also prevented it from running.

2014-11-15 Hunting / Not Hunting added

2014-10-30 Additional points were added to the display of the line of action

2014-10-22 Correction to MOW for metric helical internals

2014-10-18 Changes to the way the Tooth_Thickness_Minimum is specified when no class is used.

2014-10-15 some TextChanged were corrected to LostFocus, eg WGS Modular

2014-10-01 Correction to annotaions of EXT splines.

2014-10-08 Build 151+ LoadRegImageAlternative

2014-09-25 Added template retrieval help for AI

2014-09-05 Fix for Internal Splines, Major Diameter fit
			If specified SW cannot be started, it starts the last version.

2014-08-19 Correction  to EXT spline fillet radius when No_Class and not ANSI B92

2014-08-12 Added option for the user to specify the keyway dimensions.

2014-08-** Removed the internet time clock

2014-07-25 Master Gear Test added to data files
		   Test Radius Minimum property added 

2014 summer Bending and Sliding options were added to the Balancing Addendum Modifications

2014-07-24 WGS data file revamped

2014-07-21 Added Custom Coefficients to WGS
		   Constrain involute sketch now defaulted to true

2014-06-19 Version .132 new method for determining the end of the troichord.

2014-06-11 Change to opening GearTrax files

2014-05-27 Added contact ratio for Internal Gears that are not helical

2014-05-08 Chordal_Addendum and Chordal_Thickness properties for bevel gears added

2014-04-25 Changes to custom properties of bevel gears

2014-03-27 ASME_B29_10M_1997 & ASME_B29_15M_1997 standard added

2014-03-25 Changed the max number of spline teeth from 500 to 1001

2014-03-11  GetTrueInvoluteFormDiameter changed for external splines, there was a problem with low number of teeth  < 14

2014-02-21  Adjustment to MOW position on screen when a backlash is specified

2014-02-20  Correction to PGT tooth profiles if a backlash is specified

2014-02-14 txtSpurAddModg_LostFocus was updating the pinnion rather than the gear
